Author: Jason

FEATURES:
Accommodates PVP headsets
Custom paint colors available upon request
Approved as an open-face or full-face helmet
Stainless steel quick release buckle & reinforced chin strap
Fits most Intermediate Oval head sizes from XS - 3XL (2 shell sizes)
Kinetic Polymer Alloy shell with Multi-Density EPS and Neck Roll
Removable / washable interior
Reflective Safety Patch
Dynamic flow-through ventilation system with channeled ports
Scratch-and UV-resistant face shield with inner sun shield
Blackinton and Smith & Warren badges available upon request
Weight: 3.9 lbs / 1750 grams (approx. for size medium helmet)
5 year warranty / Meets or exceeds DOT standards

Phone: 310-212-5432
Online: www.pvpcom.com

LS2 Helmet Maintenance and Replacement
Outer Shell - Only commonly available helmet wax or plastic cleaning agents should be used to clean any dirt off the helmet’s surface. Apply sparingly to avoid damage.
Plastic Parts Including Shield - Plastic parts should not be cleaned with agents containing solvents. The shield should only be cleaned with water and a neutral cleaning agent. Heavily soiled areas can be gently cleaned using a soft toothbrush or cotton swab.
Liner & Cheek Pads - Should be removed and washed by hand or in washing net in washing machine. Fixed padding should be cleaned with neutral cleaning agent. All parts should be dried in direct sunlight.
Impact Absorption Liner (EPS) - Should be cleaned using only a damp cloth.
Helmet replacement is recommended if the helmet is subjected to an impact, the comfort padding or retention system has become loose, or there are indentiations or white scratches in the Impact Absorption Liner (EPS).

SIZE	XSM	SML	MED	LRG	XLG	2XL	3XL

SHELL	XS - XLG	2XL - 3XL

HEAD SIZE	53-54 CM	55-56 CM	57-58 CM	59-60 CM	61-62 CM	63-64 CM	65-66 CM
CHEEK PAD	XSM	SML	MED	LRG	XLG	2XL	3XL
CENTER PAD	XSM	SML	MED	LRG	XLG	2XL	3XL

Replacement Parts and Accessories Available: Sun Visor / Pinlock Shield / Pinlock Lens

Phone: 310-212-5432
Online: www.pvpcom.com